Status display-HD Encoder

HD Encoder System
Platform

# Status Display

## Input status

###

Running Time:

Device Time:(Sync Time To Device)

CPU Usage:

Memory Usage:

Input Size:

Collected Video Frames:

Lost Video Frames:

Audio Samplerate:

Net Packet Sent:

Net Packet Dropped:

## Record status

###

SD Card Status:unformart

Total Disk Space:

Free Disk Space:

Record Status:

Disk Status:Full

Disk Status:Too Slow

## DHCP status

###

IP:

Netmask:

Gateway:

## WIFI status

###

WIFI:Disable

###

WIFI status:

WIFI SSID:

WIFI IP:

WIFI MAC:

WIFI Level:

WIFI Freq:

WIFI Max Bit Rate:270 Mb/s

## 4G status

###

4G:Disable

###

4G Status:

4G IMEI：

4G Mode:

4G Level:

4G Online:

4G Rx:

4G Tx:

4G IP：

4G Gateway:

## Main stream

###

Encode Type:

Encoding Size:

Bitrate(kbit):

MJPG URL:

JPG URL:

TS URL：

HLS URL:

FLV URL:

RTSP URL:

RTMP URL:

RTMP PUSH URL:

Multicast URL:

SRT URL:

SRT PUSH URL:

Preview

## Substream1

###

Disabled (the main stream frame rate of 31~60 frames, will disable Substream)

###

Encode Type:

Encoding Size:

Bitrate(kbit):

MJPG URL:

JPG URL:

TS URL：

HLS URL:

FLV URL:

RTSP URL:

RTMP URL:

RTMP PUSH URL:

Multicast URL:

SRT URL:

SRT PUSH URL:

Preview

## Substream2

###

Disabled (the main stream frame rate of 31~60 frames, will disable Substream)

###

Encode Type:

Encoding Size:

Bitrate(kbit):

MJPG URL:

JPG URL:

TS URL：

HLS URL:

FLV URL:

RTSP URL:

RTMP URL:

RTMP PUSH URL:

Multicast URL:

SRT URL:

SRT PUSH URL:

Preview

## Substream3

###

Disabled (the main stream frame rate of 31~60 frames, will disable Substream)

###

Encode Type:

Encoding Size:

Bitrate(kbit):

MJPG URL:

JPG URL:

TS URL：

HLS URL:

FLV URL:

RTSP URL:

RTMP URL:

RTMP PUSH URL:

Multicast URL:

SRT URL:

SRT PUSH URL:

Preview