Substream3 settings-HD Encoder

HD Encoder System
Platform

# Substream3

  Disabled (the main stream frame rate of 31~60 frames, will disable Substream)

Encoding type:

FPS:
  [5-60]

GOP:
  [5-300]

Bitrate(kbit):
  [32-32000]

Encoded size:

H.264 Level:

Bitrate control:

TS URL:

HLS URL:

FLV URL:

RTSP URL:

RTMP URL:

RTMP/RTSP PUSH URL:

Multicast IP:

Multicast prot:
  [1-65535]

SRT URL Port:
  [1-65535]

SRT PUSH URL:

SRT Encryption Password:

## OSD

Alpha:
  [0-128]

### Zone 1

Zone:

Type:

X:
  [0-1920]

Y:
  [0-1080]

Text:

Font size:
  [8-72]

Background color:

Color:
  select color

Logo:

### Zone 2

Zone:

Type:

X:
  [0-1920]

Y:
  [0-1080]

Text:

Font size:
  [8-72]

Background color:

Color:
  select color

Logo:

### Zone 3

Zone:

Type:

X:
  [0-1920]

Y:
  [0-1080]

Text:

Font size:
  [8-72]

Background color:

Color:
  select color

Logo:

### Zone 4

Zone:

Type:

X:
  [0-1920]

Y:
  [0-1080]

Text:

Font size:
  [8-72]

Background color:

Color:
  select color

Logo:

### LOGO

LOGO:

  Please upload PNG or 24-bit BMP(0xF1F1F1 is transparent) pictures less than 500 kByte,
  the file name is logo1.bmp\logo2.bmp\logo3.bmp\logo4.bmp, or logo1.png\logo2.png\logo3.png\logo4.png