System settings-HD Encoder

HD Encoder System Platform
Version:

Language（语言）

## Change password

Old password:

New password:

Confirm password:

## Advanced

Device Name:

EDID:

Video Only:

Audio Only:

AV Sync Strategy:

Hls Splitter Time(s):
  [3-20]

Hls Number:
  [3-20]

SRT Latency(ms):
  [1-10000]

SRT Bandwidth(KByte, 0=nolimit):
  [0-102400]

Deinterlaced:

Net Drop Threshold:
  [50-50000]

TS muxer:

TS once pack:
  [3-128]

TS TDT:

ts_transport_stream_id:
  [1-65535]

ts_pmt_start_pid:
  [16-7936]

ts_start_pid:
  [32-3840]

ts_tables_version:
  [0-31]

ts_service_id:
  [1-65535]

ts_service_name:

ts_service_provider:

TS Empty Packet:

TS password enable:

Vmix Compatible:

TS OVER RTSP:

Multicast type:

Enable SAP:

MTU Size:
  [500-1500]

UDP TTL:
  [1-254]

UDP SOCKET_BUF_SIZE:
  (0-20971520]

Slice split enable:

Slice size:
  [128-65535]

MIN_QP:
  [1-35]

MAX_QP:
  (MIN_QP-50]

SAR(H.264 Only):

Contrast improve:
  [0-63]

Image enhance:
  [0-16]

Y space filter:
  [0-255]

Y time filter:
  [0-63]

C space filter:
  [0-255]

C time filter:
  [0-32]

## Serial to TCP

Mode:

Baud Rate:

Server Address:

Server Port:
  [1-65535]

## Schedule restart

Restart enable:

Restart time:

## NTP

NTP Enable:

NTP Server:

Time Zone:

## Upload firmware and configuration

Select File:
  (File name has to be 'up.rar' or 'box.ini'. Please don't upload by different people at the same time and don't power off during upload.)

## Backup firmware and configuration

## System settings