Main stream settings-HD Encoder

HD Encoder System Platform
Version:

Language（语言）

## Main stream

Encoding type:

FPS:

Custom FPS:
  [5-60]

GOP:
  [5-300]

Bitrate(kbit):
  [32-32000]

Image Quality:

Encoded size:

H.264 Level:

Bitrate control:

TS Video PID：
  [16-8190]

TS Audio PID：
  [16-8190]

TS URL:

HLS URL:

FLV URL:

RTSP URL:

RTSP Multicast IP:

RTSP Multicast port:
  [1-65535]

RTMP URL:

RTMP(S)/RTSP PUSH URL:

Multicast IP:

Multicast port:
  [1-65535]

Multicast SAP Name:

SRT URL Port:
  [1-65535]

SRT PUSH URL:

SRT Encryption Password:

HLS PUSH URL:

## OSD

Alpha:
  [0-255]

### Zone 1

Zone:

Type:

Position:
  [0-1080]

Speed:
  [0-30]

X：
  [0-1920]

Y：
  [0-1080]

Text:

Font size:
  [8-72]

Background color:

Color:
  select color

Logo:

### Zone 2

Zone:

Type:

X:
  [0-1920]

Y:
  [0-1080]

Text:

Font size:
  [8-72]

Background color:

Color:
  select color

Logo:

### Zone 3

Zone:

Type:

X:
  [0-1920]

Y:
  [0-1080]

Text:

Font size:
  [8-72]

Background color:

Color:
  select color

Logo:

### Zone 4

Zone:

Type:

X:
  [0-1920]

Y:
  [0-1080]

Text:

Font size:
  [8-72]

Background color:

Color:
  select color

Logo:

### LOGO

LOGO:
  (Please upload PNG or 24-bit BMP(0xF1F1F1=transparent) pictures less than 500 KB.
  The file name has to be logo1.bmp/logo2.bmp–logo4.bmp
  or logo1.png/logo2.png–logo4.png.)