Status display-HD Encoder

HD Encoder System Platform
Version:

Language（语言）

## Input status

Running Time:

Device Time: (Sync Time To Device)

Device Name:

CPU Usage:

Memory Usage:

Input Size: (VGA automatic adjustment)

Collected Video Frames:

Lost Video Frames:

Audio Samplerate:

Net Packet Sent:

Net Packet Dropped:

## DHCP status

IP:

Netmask:

Gateway:

## WIFI status

WIFI: Disable

WIFI status:

WIFI SSID:

WIFI IP:

WIFI MAC:

WIFI Level:

WIFI Freq:

WIFI Max Bit Rate: 270 Mb/s

## 4G status

4G: Disable

4G Status:

4G IMEI:

4G Mode:

4G Level:

4G Online:

4G Rx:

4G Tx:

4G IP:

4G Gateway:

## Main stream

Encode Type:

Encoding Type:

Bitrate(kbit):

MJPG URL:

JPG URL:

TS URL:

HLS URL:

FLV URL:

RTSP URL:

RTMP URL:

RTMP(S) PUSH URL:

Multicast URL:

SRT URL:

SRT PUSH URL:

Preview(HTML5)

Preview(HTML5)

## Substream1

Disabled (the main stream frame rate of 31~60 frames, will disable Substream)

Encode Type:

Encoding Type:

Bitrate(kbit):

MJPG URL:

JPG URL:

TS URL:

HLS URL:

FLV URL:

RTSP URL:

RTMP URL:

RTMP(S) PUSH URL:

Multicast URL:

SRT URL:

SRT PUSH URL:

Preview(HTML5)

Preview(HTML5)

## Substream2

Disabled (the main stream frame rate of 31~60 frames, will disable Substream)

Encode Type:

Encoding Type:

Bitrate(kbit):

MJPG URL:

JPG URL:

TS URL:

HLS URL:

FLV URL:

RTSP URL:

RTMP URL:

RTMP(S) PUSH URL:

Multicast URL:

SRT URL:

SRT PUSH URL:

Preview(HTML5)

Preview(HTML5)

## Substream3

Disabled (the main stream frame rate of 31~60 frames, will disable Substream)

Encode Type:

Encoding Type:

Bitrate(kbit):

MJPG URL:

JPG URL:

TS URL:

HLS URL:

FLV URL:

RTSP URL:

RTMP URL:

RTMP(S) PUSH URL:

Multicast URL:

SRT URL:

SRT PUSH URL:

Preview(HTML5)

Preview(HTML5)